**DECLARED VALUE OF OUR PRODUCT**

Electric Dry Iron as per IS 366:1991 & IS 302-2-3:2007, 750W/1100W, 230V, 50Hz, Single Phase ac, Thermostatically Controlled, Class-I, Ordinary, IPX0, Aluminum Alloy sole plate PTEF Coated, Pollution degree – III, Material Group IIIa/IIIb, Class of insulation E,

Rating : 230V, 50Hz, Single Phase ac,

Type : 750W/1100W, Electric Dry Iron

Grade : Class-I