**DECLARED VALUE OF OUR PRODUCT**

1. Stationary storage type Electric Water Heaters, Capacity 6 Ltr, 2000 W, 230 V 50Hz, single phase ac Closed type, drip proof, Class 1, IPX1, Pressure Class II, Rated pressure 0.6 Mpa, Pollution degree 1, Material Group IIIa, Reheating time 25 minutes (Max), Hot water output 40⁰C min, Mixing factor 45% (Max), Standing loss 0.352 kwh/day (Max), inner tank SS material Grade 304L

.

Yours faithfully

Seal:

Signature:

Designation:

Name: