**DECLARED VALUE OF OUR PRODUCT**

1. Electric Room Heater, Visibly glowing Radiant heater (Quartz) 800 W, 230V, 50 Hz, AC Single Phase, Class I, Pollution degree 1, IPX0 (Ordinary), without thermostat & Thermal cutout, as per IS 302-2-30:2007.
2. Electric Room Heater, Visibly glowing Radiant heater (Halogen) 1200 W, 230V, 50 Hz, AC Single Phase, Class I, Pollution degree 1, Class of Insulation- F, IPX0 (Ordinary), without thermostat & Thermal cutout, as per IS 302-2-30:2007.

Yours faithfully

Seal:

Signature:

Designation:

Name: