**DECLARED VALUE OF OUR PRODUCT**

1. Electric Instantaneous Water Heater, 3000 W, 230V, 50 Hz, AC Single Phase, Pollution degree 1, IPX1, Rated Pressure 0.6Mpa, Closed Type, Class 1, Stainless Steel Container, as per IS 8978:1992 & IS 302-2-35.

Yours faithfully

Seal:

Signature:

Designation:

Name:

**Works: E14 Sector: 63, Noida UP**